{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,0,9]],"flags":["formulas_cached_only"]}
["Position","Anzahl","Artikel","Herstellerbezeichnung","Hersteller","DIN-Zuordnung","SMD/THT","Lieferant"]
[{"$nulls":7},"RS","Farnell","DigiKey"]
[1,3,"100pF – 50V – 0603","06035A101JAT2A ","AVX","C1,C2,C3","SMD ",null,4766040]
[2,10,"22nF – 100V – 1206",223860115641,"Yageo","C4-13","SMD ","669-8476"]
[3,1,"TPS73033DBVR","TPS73033DBVR","Texas Instruments","IC1","SMD ",null,null,"296-17580-2-ND"]
[4,2,"MAL211838228E3","MAL211838228E3","Vishay","C14,C15","THT",null,1695286]
[5,3,"Steckverbinder 39501-1009","39501-1009","Molex","ST1,ST2,ST3","THT",null,null,"WM7758-ND"]
[6,1,"Kühlkörper 515AB1000MB","515AB1000MB","ABL Components","K1","THT","234-2514"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}