{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":7,"n_cols":8,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7]],"flags":["formulas_cached_only"]}
["DIN-Zuordnung","Artikel","Gehäuseform","Koordinaten X/mm","Koordinaten Y/mm","Rotations- grad","Bestückungs- seite (BS/LS)","SMD/THT"]
[]
["Ref-Marke 1",null,"Punkt",96.3,17,null,"BS","SMD "]
["Ref.Marke 2",null,"Punkt",5.25,55.28,null,"BS","SMD "]
["C1","100nF",603,7,17,90,"BS","SMD "]
["R2","NB","NB",15.34,18.2,0,"LS","THT"]
["IC101","74LS123",805,42.22,12.3,180,"LS","SMD "]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}